C:\Users\Darryl.SOLEX\Documents\Manufacturers Logos\Enviromist.tif

MID-DAY AND END OF DAY CLEANING

1. **Fill rinse tank with clean water and two table spoons of Dawn detergent.**
2. **Close main tank valve.**
3. **Open rinse tank valve.**
4. **Turn main switch on and run sprayer to flush the lines and CDA for at least two minutes.**

This procedure should be performed ***at least*** at noon and at the end of day. It is even better if done mid-morning and mid-afternoon also. Never leave chemical in lines and CDA head overnight.